|  |
| --- |
|  0G4A9509.jpg |

**Product Overview:**

Comes with 3 ultra-efficient thermal heat pipes. PWM air cooling solution powered by Heat Core Touch Technology (HCTT) and equipped with high efficiency fins. Compatible with most current motherboard designs.

**Specifications**

|  |  |
| --- | --- |
| Model  | Verkho 3 |
| Base Material | Aluminum block with HCTT Heat Core Touch Technology |
| Fin Material | Aluminum |
| Heat pipe | 6mm x 3 |
| Dimension | 120 x 81 x 122.5mm |
| TDP(Thermal Design Power) | 120 |
| Fan | Speed | 1200-2800 rpm  |
| Connector | PWM 4-Pin |
| Dimension | 90 x 90 x 25mm |
| Bearing Type | Hydraulic Bearing |
| Started Voltage | 5V |
| Rated Voltage | 12V |
| Rated Current | 0.2 A  |
| Power Consumption | 2.4 Watts |
| Air Pressure | 0.548-1.24 mm-H2O |
| Air Flow | 18.9-45.5 CFM |
| Noise | 15-24 dBA |
| MTBF (Mean Time Before Failure) | 60000 hrs. |
| Socket | LGA 1156/1155/1151/1150/775 AM4/AM3+/AM3/AM2+/AM2/FM2/FM1 |

**Warranty**

1 year

**Features**

* TDP (Thermal Design Power) up to 120W.
* Compact side flow air cooler for maximum compatibility.
* Heat Core Touch Technology and 3 ultra-efficient thermal heat pipes.
* Upgraded high efficiency fins for optimal thermal performance.
* Ultra-slim profile capable of mounting single 90mm fan configurations; works with most current motherboard designs.

**Package Information**

|  |  |  |  |
| --- | --- | --- | --- |
| **Product Name** | **Product Number** | **EAN CODE** | **UPC CODE** |
| Verkho 3 |  |  |  |
|  |  |  |  |
| **Carton Size ( L x W x H )** | 425 x 330 x 365 mm | **Carton Weight**  |  |
| **Retail Box Size ( L x W x H )** | 135 x 104 x 175 mm | **Retail Box Weight**  |  |
| **Carton Qty** | 18 pcs | **Pallet Qty** |  |