|  |
| --- |
| 12.jpg |

**Product Overview:**

Air cooling solution with 3-Pin connector. Comes equipped with high efficiency fins and compact profile. Compatible with most current AMD motherboard designs. **Only for AMD chipset configurations.**

**Specifications**

|  |  |  |
| --- | --- | --- |
| Model | | Verkho A-3P |
| Base Material | | Aluminum |
| Dimension | | 112 x 112 x 55mm |
| TDP(Thermal Design Power) | | 100 |
| Fan | Speed | 2300 rpm |
| Connector | 3-Pin |
| Dimension | 90 x 90 x 25mm |
| Bearing Type | Hydraulic Bearing |
| Started Voltage | 6V |
| Rated Voltage | 12V |
| Rated Current | 0.24 A |
| Power Consumption | 2.88 Watts (One Fan) |
| Air Pressure | 1.34 mm-H2O |
| Air Flow | 61.32 CFM |
| Noise | 28.9dBA |
| MTBF  (Mean Time Before Failure) | 60000 hrs. |
| Socket | | AM4/AM3+/AM3/AM2+/AM2/ FM2/FM1 |

**Warranty**

1 year

**Features**

* TDP (Thermal Design Power) up to 100W.
* Upgraded high efficiency fins for optimal thermal performance.
* Compact profile capable of mounting single 90mm fan configurations; works with most current AMD motherboard designs. **Only for AMD chipset configurations.**

**Package Information**

|  |  |  |  |
| --- | --- | --- | --- |
| **Product Name** | **Product Number** | **EAN CODE** | **UPC CODE** |
| Verkho A-3P |  |  |  |
|  |  |  |  |
| **Carton Size ( L x W x H )** | 625 x 375 x 280 mm | **Carton Weight** | N.W 14.8 kg / G.W 16.2 kg |
| **Retail Box Size ( L x W x H )** | 120 x 120 x 65 mm | **Retail Box Weight** | N.W 199 g / G.W 248 g |
| **Carton Qty** | 60 pcs | **Pallet Qty** | 1680(GP)/2160(HQ) |