|  |
| --- |
| 8.jpg |

**Product Overview:**

Universal air cooling solution compatible with most current AMD and Intel motherboard designs. Equipped with high efficiency fins and compact profile. **Not compatible with Intel 2011 and 2066.**

**Specifications**

|  |  |  |
| --- | --- | --- |
| Model | | BAS U-3P |
| Base Material | | Aluminum |
| Dimension | | 131 x 131 x 62mm |
| TDP(Thermal Design Power) | | 110 |
| Fan | Speed | 1800 rpm |
| Connector | 3-Pin |
| Dimension | 120 x 120 x 25mm |
| Bearing Type | Hydraulic Bearing |
| Started Voltage | 5V |
| Rated Voltage | 12V |
| Rated Current | 0.3 A |
| Power Consumption | 3.6 Watts |
| Air Pressure | 1.22 mm-H2O |
| Air Flow | 59.8 CFM |
| Noise | 26.3dBA |
| MTBF (Mean Time Before Failure) | 60000 hrs. |
| Socket | | LGA 1156/1155/1151/1150/775 AM4/AM3+/AM3/AM2+/AM2/FM2/FM1 |

**Warranty**

1 year

**Features**

* TDP (Thermal Design Power) up to 110W.
* Upgraded high efficiency fins with maximum thermal performance.
* Compact profile capable of mounting single 120mm fan configurations; works with most current AMD and Intel motherboard designs. **Not compatible with Intel 2011 and 2066.**

**Package Information**

|  |  |  |  |
| --- | --- | --- | --- |
| **Product Name** | **Product Number** | **EAN CODE** | **UPC CODE** |
| BAS U-3P |  |  |  |
|  |  |  |  |
| **Carton Size ( L x W x H )** | 566 x 430 x 380 mm | **Carton Weight** |  |
| **Retail Box Size ( L x W x H )** |  | **Retail Box Weight** |  |
| **Carton Qty** | 60 pcs | **Pallet Qty** |  |